**AIP Cameras**

All IP cam Wifi security key: science12345

Camera Access, View Only: User science; Password = 12345

IP Maintenance Port LAN settings = IP = 192.168.2.170 mask = 255.255.255.0 gateway = 192.168.2.1

IP Cameras  
# Name IP Address Video Camera

# - Port Mast 192.168.17.2 Not Installed

# - STBD Mast 192.168.17.3 Not Installed

# 5 –Dog House 192.168.17.4 H.264 SC384

# 2 - Port Boom 192.168.17.5 MPEG-4 NS202A

# 3 - STBD Deck 192.168.17.6 MPEG-4 NS202A

# 14 - Bow Thruster 192.168.17.7 MPEG-4 NS202A

# 7 - Hydro Winch FWD 192.168.17.9 H.264 SC386

# 6 - Hydro Winch AFT 192.168.17.10 H.264 SC386

# 10 - Winch HPU Ctr 192.168.17.17 MPEG-4 NS202A

# 9 - Fiber Winch 192.168.17.18 MPEG-4 NS202A

# 12 - Trawl Winch 192.168.17.19 MPEG-4 NS202A

#13 - Aft Propulsion 192.168.17.20 MPEG-4 NS202A

#11 - A-Frame ……….. 192.168.17.21 Moog

#8 - HYRO Boom ….. 192.168.17.23 MJPEG SC384

#11 Traction Head …… 192.168.17.22 MJPEG NW484

Network Video Recorder (NVR) … 192.168.17.249 WJ-NV200

MAINLABCAM WIFI 192.168.1.11 Linksys E4200

DOGHOUSECAM WIFI 192.168.1.12 Linksys E4200

CHARTRMIPCAMS WIFI 192.168.1.13 Linksys E4200

LVL03IPCAMS WIFI 192.168.1.14 Linksys E4200

IP camera Network settings

IP: 192.168.17.200

Subnet: 255.255.255.0