Transducer Connection – Male pins Pur= Ground Pin, Yel= 12kHz, Org=34kHz

1

2

3

Impulse Connector – Female pins

1

2

3

Transducer Well Jbox In

BlackWhite Green Red

Transducer Well Jbox Out

Black White Green

Lab Terminal Strips

Green White Black

“Microphone” Receptacle – Male pins

2

1

3

“Microphone” Plug – Female pins

1

2

3

Plug into Knudsen 320B/R – Male pins Plug into Knudsen 3260 – Male pins

A

C

B

Knudsen 12kHz In – Female pins Pur=Signal-, Yel= Signal+, Org=Shield

320

3260

C

A

C

B

B

A